In PCLake, wind drink resuspension, not flowrate driven resuspension in our system

Very high concentration measured by wind-driven accumulation.

Short wave

Sobek at seconds. Asking output of Sobek from Thomas.

Assume e to be 0.

Turbidity data from HydroNet (South of Breda), Turbidity vs discharge.

Summer very low discharge, no resuspension effect